# Static Call Graph for image .\Objects\labtemplateea.axf

#<CALLGRAPH># ARM Linker, 5060061: Last Updated: Fri Oct 18 12:50:44 2024

### Maximum Stack Usage = 232 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

LPTMR0_IRQHandler ⇒ fprint ⇒ debug_printf ⇒ _doprint ⇒ fput_pad

### Functions with no stack information

- asmmain
- LPTMR0_IRQHandler
- asm_low_power_timer_interrupt_request

### Mutually Recursive functions

- NMI_Handler ⇒ NMI_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- SVC_Handler ⇒ SVC_Handler
- DebugMon_Handler ⇒ DebugMon_Handler
- PendSV_Handler ⇒ PendSV_Handler
- SysTick_Handler ⇒ SysTick_Handler

  ### Function Pointers

  - ADC0_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - ADC1_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - BusFault_Handler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - CAN0_Bus_Off_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - CAN0_Error_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - CAN0_ORed_Message_buffer_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - CAN0_Rx_Warning_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - CAN0_Tx_Warning_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - CAN0_Wake_Up_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - CAN1_Bus_Off_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - CAN1_Error_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - CAN1_ORed_Message_buffer_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - CAN1_Rx_Warning_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - CAN1_Tx_Warning_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - CAN1_Wake_Up_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - CLOCK_SYS_FllStableDelay from fsl_clock_mk60d10.o(i.CLOCK_SYS_FllStableDelay) referenced from fsl_clock_mk60d10.o(i.CLOCK_SYS_SetConfiguration)
  - CMP0_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - CMP1_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - CMP2_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - CMT_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - DAC0_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - DAC1_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - DMA0_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - DMA10_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - DMA11_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - DMA12_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - DMA13_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - DMA14_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - DMA15_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - DMA1_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - DMA2_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - DMA3_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - DMA4_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - DMA5_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - DMA6_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - DMA7_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - DMA8_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - DMA9_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - DMA_Error_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - DebugMon_Handler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - DefaultISR from startup_mk60d10.o(.text) referenced 135 times from startup_mk60d10.o(RESET)
  - ENET_1588_Timer_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - ENET_Error_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - ENET_Receive_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - ENET_Transmit_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - FTFL_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - FTM0_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - FTM1_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - FTM2_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - HardFault_Handler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - I2C0_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - I2C1_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - I2S0_Rx_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - I2S0_Tx_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - LLWU_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - LPTMR0_IRQHandler from my_main.o(MyCode) referenced from startup_mk60d10.o(RESET)
  - LVD_LVW_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - MCG_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - MCM_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - MemManage_Handler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - NMI_Handler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - PDB0_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - PIT0_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - PIT1_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - PIT2_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - PIT3_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - PORTA_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - PORTB_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - PORTC_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - PORTD_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - PORTE_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - PendSV_Handler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - RNG_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - RTC_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - RTC_Seconds_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - Read_Collision_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - Reserved102_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - Reserved108_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - Reserved109_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - Reserved111_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - Reserved112_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - Reserved113_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - Reserved114_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - Reserved115_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - Reserved116_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - Reserved117_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - Reserved118_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - Reserved119_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - Reserved59_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - Reserved95_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - Reset_Handler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - SDHC_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - SPI0_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - SPI1_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - SPI2_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - SVC_Handler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - SWI_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - SysTick_Handler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - SystemInit from system_mk60d10.o(i.SystemInit) referenced from startup_mk60d10.o(.text)
  - TSI0_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - UART0_ERR_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - UART0_LON_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - UART0_RX_TX_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - UART1_ERR_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - UART1_RX_TX_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - UART2_ERR_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - UART2_RX_TX_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - UART3_ERR_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - UART3_RX_TX_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - UART4_ERR_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - UART4_RX_TX_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - UART5_ERR_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - UART5_RX_TX_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - UART_HAL_ReceiveDataPolling from fsl_uart_hal.o(i.UART_HAL_ReceiveDataPolling) referenced from fsl_debug_console.o(i.DbgConsole_Init)
  - UART_HAL_SendDataPolling from fsl_uart_hal.o(i.UART_HAL_SendDataPolling) referenced from fsl_debug_console.o(i.DbgConsole_Init)
  - USB0_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - USBDCD_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - UsageFault_Handler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - WDOG_EWM_IRQHandler from startup_mk60d10.o(.text) referenced from startup_mk60d10.o(RESET)
  - __main from __main.o(!!!main) referenced from startup_mk60d10.o(.text)
  - _printf_input_char from _printf_char_common.o(.text) referenced from _printf_char_common.o(.text)
  - debug_putc from fsl_debug_console.o(i.debug_putc) referenced from fsl_debug_console.o(i.debug_printf)
  - fputc from fsl_debug_console.o(i.fputc) referenced from _printf_char_file.o(.text)
  - init_data_bss from startup.o(i.init_data_bss) referenced from startup_mk60d10.o(.text)

  ### Global Symbols

  __main (Thumb, 8 bytes, Stack size 0 bytes, __main.o(!!!main))
  [Calls]

  - >> __scatterload
  - >> __rt_entry

  __scatterload (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter))
  [Called By]

  - >> __main

  __scatterload_rt2 (Thumb, 44 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)
  [Calls]

  - >> __rt_entry

  __scatterload_rt2_thumb_only (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_null (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_copy (Thumb, 26 bytes, Stack size unknown bytes, __scatter_copy.o(!!handler_copy), UNUSED)
  [Calls]

  - >> __scatterload_copy
  [Called By]
  - >> __scatterload_copy

  __scatterload_zeroinit (Thumb, 28 bytes, Stack size unknown bytes, __scatter_zi.o(!!handler_zi), UNUSED)

  _printf_d (Thumb, 0 bytes, Stack size unknown bytes, _printf_d.o(.ARM.Collect$$_printf_percent$$00000009))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = _printf_d ⇒ _printf_int_dec ⇒ _printf_int_common
  [Calls]
  - >> _printf_int_dec

  _printf_percent (Thumb, 0 bytes, Stack size unknown bytes, _printf_percent.o(.ARM.Collect$$_printf_percent$$00000000))
  [Called By]

  - >> __printf

  _printf_s (Thumb, 0 bytes, Stack size unknown bytes, _printf_s.o(.ARM.Collect$$_printf_percent$$00000014))
  [Stack]

  - Max Depth = 24 + Unknown Stack Size
  - Call Chain = _printf_s ⇒ _printf_string ⇒ _printf_cs_common ⇒ _printf_str
  [Calls]
  - >> _printf_string

  _printf_percent_end (Thumb, 0 bytes, Stack size unknown bytes, _printf_percent_end.o(.ARM.Collect$$_printf_percent$$00000017))

  __rt_lib_init (Thumb, 0 bytes, Stack size unknown bytes, libinit.o(.ARM.Collect$$libinit$$00000000))
  [Called By]

  - >> __rt_entry_li

  __rt_lib_init_alloca_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002E))

  __rt_lib_init_argv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002C))

  __rt_lib_init_atexit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001B))

  __rt_lib_init_clock_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000021))

  __rt_lib_init_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000032))

  __rt_lib_init_exceptions_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000030))

  __rt_lib_init_fp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000002))

  __rt_lib_init_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001F))

  __rt_lib_init_getenv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000023))

  __rt_lib_init_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000A))

  __rt_lib_init_lc_collate_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000011))

  __rt_lib_init_lc_ctype_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000013))

  __rt_lib_init_lc_monetary_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000015))

  __rt_lib_init_lc_numeric_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000017))

  __rt_lib_init_lc_time_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000019))

  __rt_lib_init_preinit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000004))

  __rt_lib_init_rand_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000E))

  __rt_lib_init_return (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000033))

  __rt_lib_init_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001D))

  __rt_lib_init_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000025))

  __rt_lib_init_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000C))

  __rt_lib_shutdown (Thumb, 0 bytes, Stack size unknown bytes, libshutdown.o(.ARM.Collect$$libshutdown$$00000000))
  [Called By]

  - >> __rt_exit_ls

  __rt_lib_shutdown_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000002))

  __rt_lib_shutdown_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000007))

  __rt_lib_shutdown_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000F))

  __rt_lib_shutdown_return (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000010))

  __rt_lib_shutdown_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000A))

  __rt_lib_shutdown_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000004))

  __rt_lib_shutdown_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000C))

  __rt_entry (Thumb, 0 bytes, Stack size unknown bytes, __rtentry.o(.ARM.Collect$$rtentry$$00000000))
  [Called By]

  - >> __scatterload_rt2
  - >> __main

  __rt_entry_presh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000002))

  __rt_entry_sh (Thumb, 0 bytes, Stack size unknown bytes, __rtentry7.o(.ARM.Collect$$rtentry$$00000007))

  __rt_entry_li (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000A))
  [Calls]

  - >> __rt_lib_init

  __rt_entry_postsh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000009))

  __rt_entry_main (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000D))
  [Stack]

  - Max Depth = 232 + Unknown Stack Size
  - Call Chain = __rt_entry_main ⇒ main ⇒ debug_printf ⇒ _doprint ⇒ fput_pad
  [Calls]
  - >> exit
  - >> main

  __rt_entry_postli_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000C))

  __rt_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit.o(.ARM.Collect$$rtexit$$00000000))
  [Called By]

  - >> exit

  __rt_exit_ls (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000003))
  [Calls]

  - >> __rt_lib_shutdown

  __rt_exit_prels_1 (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000002))

  __rt_exit_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000004))
  [Calls]

  - >> _sys_exit

  Reset_Handler (Thumb, 18 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - startup_mk60d10.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_mk60d10.o(RESET)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_mk60d10.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_mk60d10.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_mk60d10.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler
  [Address Reference Count : 1]
  - startup_mk60d10.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Calls]

  - >> DebugMon_Handler
  [Called By]
  - >> DebugMon_Handler
  [Address Reference Count : 1]
  - startup_mk60d10.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - startup_mk60d10.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Calls]

  - >> SysTick_Handler
  [Called By]
  - >> SysTick_Handler
  [Address Reference Count : 1]
  - startup_mk60d10.o(RESET)

  ADC0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Calls]

  - >> DefaultISR
  [Address Reference Count : 1]
  - startup_mk60d10.o(RESET)

  ADC1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  CAN0_Bus_Off_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  CAN0_Error_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  CAN0_ORed_Message_buffer_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  CAN0_Rx_Warning_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  CAN0_Tx_Warning_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  CAN0_Wake_Up_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  CAN1_Bus_Off_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  CAN1_Error_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  CAN1_ORed_Message_buffer_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  CAN1_Rx_Warning_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  CAN1_Tx_Warning_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  CAN1_Wake_Up_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  CMP0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  CMP1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  CMP2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  CMT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  DAC0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  DAC1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  DMA0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  DMA10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  DMA11_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  DMA12_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  DMA13_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  DMA14_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  DMA15_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  DMA1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  DMA2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  DMA3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  DMA4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  DMA5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  DMA6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  DMA7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  DMA8_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  DMA9_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  DMA_Error_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  DefaultISR (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Called By]

  - >> ADC0_IRQHandler
  [Address Reference Count : 1]
  - startup_mk60d10.o(RESET)

  ENET_1588_Timer_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  ENET_Error_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  ENET_Receive_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  ENET_Transmit_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  FTFL_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  FTM0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  FTM1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  FTM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  I2C0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  I2C1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  I2S0_Rx_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  I2S0_Tx_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  LLWU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  LVD_LVW_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  MCG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  MCM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  PDB0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  PIT0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  PIT1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  PIT2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  PIT3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  PORTA_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  PORTB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  PORTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  PORTD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  PORTE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  RNG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  RTC_Seconds_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  Read_Collision_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  Reserved102_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  Reserved108_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  Reserved109_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  Reserved111_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  Reserved112_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  Reserved113_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  Reserved114_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  Reserved115_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  Reserved116_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  Reserved117_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  Reserved118_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  Reserved119_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  Reserved59_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  Reserved95_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  SDHC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  SPI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  SWI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  TSI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  UART0_ERR_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  UART0_LON_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  UART0_RX_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  UART1_ERR_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  UART1_RX_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  UART2_ERR_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  UART2_RX_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  UART3_ERR_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  UART3_RX_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  UART4_ERR_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  UART4_RX_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  UART5_ERR_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  UART5_RX_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  USB0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  USBDCD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  WDOG_EWM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_mk60d10.o(.text))
  [Address Reference Count : 1]

  - startup_mk60d10.o(RESET)

  __2printf (Thumb, 20 bytes, Stack size 24 bytes, noretval__2printf.o(.text))
  [Stack]

  - Max Depth = 128 + Unknown Stack Size
  - Call Chain = __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> _printf_char_file
  [Called By]
  - >> __aeabi_assert

  __printf (Thumb, 104 bytes, Stack size 24 bytes, __printf.o(.text))
  [Stack]

  - Max Depth = 24 + Unknown Stack Size
  - Call Chain = __printf
  [Calls]
  - >> _printf_percent
  [Called By]
  - >> _printf_char_common

  _printf_str (Thumb, 82 bytes, Stack size 16 bytes, _printf_str.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = _printf_str
  [Called By]
  - >> _printf_cs_common

  _printf_int_dec (Thumb, 104 bytes, Stack size 24 bytes, _printf_dec.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = _printf_int_dec ⇒ _printf_int_common
  [Calls]
  - >> _printf_int_common
  [Called By]
  - >> _printf_d

  strlen (Thumb, 62 bytes, Stack size 8 bytes, strlen.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = strlen
  [Called By]
  - >> _doprint

  __aeabi_memcpy4 (Thumb, 0 bytes, Stack size 8 bytes, rt_memcpy_w.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __aeabi_memcpy4
  [Called By]
  - >> DbgConsole_Init

  __aeabi_memcpy8 (Thumb, 0 bytes, Stack size 8 bytes, rt_memcpy_w.o(.text), UNUSED)

  __rt_memcpy_w (Thumb, 100 bytes, Stack size 8 bytes, rt_memcpy_w.o(.text), UNUSED)

  _memcpy_lastbytes_aligned (Thumb, 0 bytes, Stack size unknown bytes, rt_memcpy_w.o(.text), UNUSED)

  _printf_int_common (Thumb, 178 bytes, Stack size 32 bytes, _printf_intcommon.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = _printf_int_common
  [Called By]
  - >> _printf_int_dec

  _printf_cs_common (Thumb, 20 bytes, Stack size 8 bytes, _printf_char.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = _printf_cs_common ⇒ _printf_str
  [Calls]
  - >> _printf_str
  [Called By]
  - >> _printf_string
  - >> _printf_char

  _printf_char (Thumb, 16 bytes, Stack size 0 bytes, _printf_char.o(.text), UNUSED)
  [Calls]

  - >> _printf_cs_common

  _printf_string (Thumb, 8 bytes, Stack size 0 bytes, _printf_char.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = _printf_string ⇒ _printf_cs_common ⇒ _printf_str
  [Calls]
  - >> _printf_cs_common
  [Called By]
  - >> _printf_s

  _printf_char_file (Thumb, 32 bytes, Stack size 16 bytes, _printf_char_file.o(.text))
  [Stack]

  - Max Depth = 104 + Unknown Stack Size
  - Call Chain = _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> ferror
  - >> _printf_char_common
  [Called By]
  - >> __2printf

  _printf_char_common (Thumb, 32 bytes, Stack size 64 bytes, _printf_char_common.o(.text))
  [Stack]

  - Max Depth = 88 + Unknown Stack Size
  - Call Chain = _printf_char_common ⇒ __printf
  [Calls]
  - >> __printf
  [Called By]
  - >> _printf_char_file

  ferror (Thumb, 8 bytes, Stack size 0 bytes, ferror.o(.text))
  [Called By]

  - >> _printf_char_file

  __I$use$semihosting (Thumb, 0 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __use_no_semihosting_swi (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __semihosting_library_function (Thumb, 0 bytes, Stack size 8 bytes, indicate_semi.o(.text), UNUSED)

  exit (Thumb, 18 bytes, Stack size 8 bytes, exit.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = exit
  [Calls]
  - >> __rt_exit
  [Called By]
  - >> __rt_entry_main

  _sys_exit (Thumb, 8 bytes, Stack size 0 bytes, sys_exit.o(.text))
  [Called By]

  - >> __rt_exit_exit

  asmmain (Thumb, 0 bytes, Stack size unknown bytes, my_main.o(MyCode))
  [Called By]

  - >> main

  LPTMR0_IRQHandler (Thumb, 0 bytes, Stack size unknown bytes, my_main.o(MyCode))
  [Stack]

  - Max Depth = 232 + Unknown Stack Size
  - Call Chain = LPTMR0_IRQHandler ⇒ fprint ⇒ debug_printf ⇒ _doprint ⇒ fput_pad
  [Calls]
  - >> fprint
  [Address Reference Count : 1]
  - startup_mk60d10.o(RESET)

  asm_low_power_timer_interrupt_request (Thumb, 0 bytes, Stack size unknown bytes, my_main.o(MyCode), UNUSED)

  BOARD_ClockInit (Thumb, 46 bytes, Stack size 8 bytes, board.o(i.BOARD_ClockInit))
  [Stack]

  - Max Depth = 192 + Unknown Stack Size
  - Call Chain = BOARD_ClockInit ⇒ BOARD_InitRtcOsc ⇒ CLOCK_SYS_RtcOscInit ⇒ __aeabi_assert ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> CLOCK_SYS_SetConfiguration
  - >> BOARD_InitRtcOsc
  - >> BOARD_InitOsc0
  - >> PORT_HAL_SetMuxMode
  [Called By]
  - >> hardware_init

  BOARD_InitOsc0 (Thumb, 20 bytes, Stack size 24 bytes, board.o(i.BOARD_InitOsc0))
  [Stack]

  - Max Depth = 184 + Unknown Stack Size
  - Call Chain = BOARD_InitOsc0 ⇒ CLOCK_SYS_OscInit ⇒ __aeabi_assert ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> CLOCK_SYS_OscInit
  [Called By]
  - >> BOARD_ClockInit

  BOARD_InitRtcOsc (Thumb, 20 bytes, Stack size 16 bytes, board.o(i.BOARD_InitRtcOsc))
  [Stack]

  - Max Depth = 184 + Unknown Stack Size
  - Call Chain = BOARD_InitRtcOsc ⇒ CLOCK_SYS_RtcOscInit ⇒ __aeabi_assert ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> CLOCK_SYS_RtcOscInit
  [Called By]
  - >> BOARD_ClockInit

  CLOCK_HAL_EnablePll0InFllMode (Thumb, 64 bytes, Stack size 12 bytes, fsl_mcg_hal.o(i.CLOCK_HAL_EnablePll0InFllMode))
  [Stack]

  - Max Depth = 12
  - Call Chain = CLOCK_HAL_EnablePll0InFllMode
  [Called By]
  - >> CLOCK_SYS_SetMcgMode

  CLOCK_HAL_GetFllClk (Thumb, 82 bytes, Stack size 24 bytes, fsl_mcg_hal.o(i.CLOCK_HAL_GetFllClk))
  [Stack]

  - Max Depth = 68
  - Call Chain = CLOCK_HAL_GetFllClk ⇒ CLOCK_HAL_GetFllRefClk ⇒ CLOCK_HAL_TestFllExternalRefFreq
  [Calls]
  - >> CLOCK_HAL_TestFllFreq
  - >> CLOCK_HAL_GetFllRefClk
  [Called By]
  - >> CLOCK_HAL_GetOutClk

  CLOCK_HAL_GetFllRefClk (Thumb, 80 bytes, Stack size 32 bytes, fsl_mcg_hal.o(i.CLOCK_HAL_GetFllRefClk))
  [Stack]

  - Max Depth = 44
  - Call Chain = CLOCK_HAL_GetFllRefClk ⇒ CLOCK_HAL_TestFllExternalRefFreq
  [Calls]
  - >> CLOCK_HAL_TestFllExternalRefFreq
  - >> CLOCK_HAL_GetMcgExternalClkFreq
  [Called By]
  - >> CLOCK_HAL_GetFllClk

  CLOCK_HAL_GetInternalRefClk (Thumb, 52 bytes, Stack size 0 bytes, fsl_mcg_hal.o(i.CLOCK_HAL_GetInternalRefClk))
  [Called By]

  - >> CLOCK_HAL_GetOutClk

  CLOCK_HAL_GetMcgMode (Thumb, 150 bytes, Stack size 32 bytes, fsl_mcg_hal_modes.o(i.CLOCK_HAL_GetMcgMode))
  [Stack]

  - Max Depth = 32
  - Call Chain = CLOCK_HAL_GetMcgMode
  [Calls]
  - >> CLOCK_HAL_IsPllSelected
  - >> CLOCK_HAL_GetFllSrc
  - >> CLOCK_HAL_GetClkOutStat
  [Called By]
  - >> CLOCK_HAL_SetPbeMode
  - >> CLOCK_HAL_SetFbiMode
  - >> CLOCK_HAL_SetFbeMode
  - >> CLOCK_SYS_SetMcgMode

  CLOCK_HAL_GetOutClk (Thumb, 78 bytes, Stack size 16 bytes, fsl_mcg_hal.o(i.CLOCK_HAL_GetOutClk))
  [Stack]

  - Max Depth = 84
  - Call Chain = CLOCK_HAL_GetOutClk ⇒ CLOCK_HAL_GetFllClk ⇒ CLOCK_HAL_GetFllRefClk ⇒ CLOCK_HAL_TestFllExternalRefFreq
  [Calls]
  - >> CLOCK_HAL_GetPll0Clk
  - >> CLOCK_HAL_GetInternalRefClk
  - >> CLOCK_HAL_GetFllClk
  - >> CLOCK_HAL_GetMcgExternalClkFreq
  [Called By]
  - >> CLOCK_SYS_GetSystemClockFreq
  - >> CLOCK_SYS_GetCoreClockFreq
  - >> CLOCK_SYS_GetBusClockFreq

  CLOCK_HAL_GetPll0Clk (Thumb, 68 bytes, Stack size 16 bytes, fsl_mcg_hal.o(i.CLOCK_HAL_GetPll0Clk))
  [Stack]

  - Max Depth = 32
  - Call Chain = CLOCK_HAL_GetPll0Clk ⇒ CLOCK_HAL_GetPll0RefFreq ⇒ CLOCK_HAL_GetMcgExternalClkFreq
  [Calls]
  - >> CLOCK_HAL_GetPll0RefFreq
  [Called By]
  - >> CLOCK_HAL_GetOutClk

  CLOCK_HAL_GetPll0RefFreq (Thumb, 12 bytes, Stack size 8 bytes, fsl_mcg_hal.o(i.CLOCK_HAL_GetPll0RefFreq))
  [Stack]

  - Max Depth = 16
  - Call Chain = CLOCK_HAL_GetPll0RefFreq ⇒ CLOCK_HAL_GetMcgExternalClkFreq
  [Calls]
  - >> CLOCK_HAL_GetMcgExternalClkFreq
  [Called By]
  - >> CLOCK_HAL_GetPll0Clk

  CLOCK_HAL_SetFbeMode (Thumb, 236 bytes, Stack size 40 bytes, fsl_mcg_hal_modes.o(i.CLOCK_HAL_SetFbeMode))
  [Stack]

  - Max Depth = 72
  - Call Chain = CLOCK_HAL_SetFbeMode ⇒ CLOCK_HAL_GetMcgMode
  [Calls]
  - >> CLOCK_HAL_GetMcgMode
  - >> CLOCK_HAL_IsPllSelected
  - >> CLOCK_HAL_IsOsc0Stable
  - >> CLOCK_HAL_GetFllSrc
  - >> CLOCK_HAL_GetClkOutStat
  - >> CLOCK_HAL_TestOscFreq
  [Called By]
  - >> CLOCK_SYS_SetMcgMode

  CLOCK_HAL_SetFbiMode (Thumb, 170 bytes, Stack size 32 bytes, fsl_mcg_hal_modes.o(i.CLOCK_HAL_SetFbiMode))
  [Stack]

  - Max Depth = 64
  - Call Chain = CLOCK_HAL_SetFbiMode ⇒ CLOCK_HAL_GetMcgMode
  [Calls]
  - >> CLOCK_HAL_UpdateFastClkInternalRefDiv
  - >> CLOCK_HAL_GetMcgMode
  - >> CLOCK_HAL_GetInternalRefClkMode
  - >> CLOCK_HAL_GetFllSrc
  - >> CLOCK_HAL_GetClkOutStat
  [Called By]
  - >> CLOCK_SYS_SetMcgMode

  CLOCK_HAL_SetOsc0Mode (Thumb, 36 bytes, Stack size 12 bytes, fsl_mcg_hal.o(i.CLOCK_HAL_SetOsc0Mode))
  [Stack]

  - Max Depth = 12
  - Call Chain = CLOCK_HAL_SetOsc0Mode
  [Called By]
  - >> CLOCK_SYS_OscInit

  CLOCK_HAL_SetOutDiv (Thumb, 56 bytes, Stack size 16 bytes, fsl_sim_hal_mk60d10.o(i.CLOCK_HAL_SetOutDiv))
  [Stack]

  - Max Depth = 16
  - Call Chain = CLOCK_HAL_SetOutDiv
  [Called By]
  - >> CLOCK_SYS_SetConfiguration
  - >> CLOCK_SYS_SetSimConfigration

  CLOCK_HAL_SetPbeMode (Thumb, 228 bytes, Stack size 40 bytes, fsl_mcg_hal_modes.o(i.CLOCK_HAL_SetPbeMode))
  [Stack]

  - Max Depth = 72
  - Call Chain = CLOCK_HAL_SetPbeMode ⇒ CLOCK_HAL_GetMcgMode
  [Calls]
  - >> CLOCK_HAL_GetMcgMode
  - >> CLOCK_HAL_PrepareOsc
  - >> CLOCK_HAL_IsPllSelected
  - >> CLOCK_HAL_GetClkOutStat
  - >> CLOCK_HAL_TestOscFreq
  [Called By]
  - >> CLOCK_SYS_SetMcgMode

  CLOCK_HAL_TestFllExternalRefFreq (Thumb, 70 bytes, Stack size 12 bytes, fsl_mcg_hal.o(i.CLOCK_HAL_TestFllExternalRefFreq))
  [Stack]

  - Max Depth = 12
  - Call Chain = CLOCK_HAL_TestFllExternalRefFreq
  [Called By]
  - >> CLOCK_HAL_GetFllRefClk

  CLOCK_HAL_TestFllFreq (Thumb, 50 bytes, Stack size 8 bytes, fsl_mcg_hal.o(i.CLOCK_HAL_TestFllFreq))
  [Stack]

  - Max Depth = 8
  - Call Chain = CLOCK_HAL_TestFllFreq
  [Called By]
  - >> CLOCK_HAL_GetFllClk

  CLOCK_HAL_TestOscFreq (Thumb, 30 bytes, Stack size 0 bytes, fsl_mcg_hal.o(i.CLOCK_HAL_TestOscFreq))
  [Called By]

  - >> CLOCK_HAL_SetPbeMode
  - >> CLOCK_HAL_SetFbeMode
  - >> CLOCK_HAL_GetMcgExternalClkFreq

  CLOCK_HAL_UpdateFastClkInternalRefDiv (Thumb, 104 bytes, Stack size 16 bytes, fsl_mcg_hal.o(i.CLOCK_HAL_UpdateFastClkInternalRefDiv))
  [Stack]

  - Max Depth = 16
  - Call Chain = CLOCK_HAL_UpdateFastClkInternalRefDiv
  [Calls]
  - >> CLOCK_HAL_SetInternalRefClkMode
  - >> CLOCK_HAL_GetInternalRefClkMode
  [Called By]
  - >> CLOCK_HAL_SetFbiMode
  - >> CLOCK_SYS_SetMcgMode

  CLOCK_SYS_EnablePortClock (Thumb, 34 bytes, Stack size 8 bytes, fsl_clock_mk60d10.o(i.CLOCK_SYS_EnablePortClock))
  [Stack]

  - Max Depth = 152 + Unknown Stack Size
  - Call Chain = CLOCK_SYS_EnablePortClock ⇒ __aeabi_assert ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> __aeabi_assert
  - >> SIM_HAL_EnableClock
  [Called By]
  - >> hardware_init

  CLOCK_SYS_EnableUartClock (Thumb, 34 bytes, Stack size 8 bytes, fsl_clock_mk60d10.o(i.CLOCK_SYS_EnableUartClock))
  [Stack]

  - Max Depth = 152 + Unknown Stack Size
  - Call Chain = CLOCK_SYS_EnableUartClock ⇒ __aeabi_assert ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> __aeabi_assert
  - >> SIM_HAL_EnableClock
  [Called By]
  - >> DbgConsole_Init

  CLOCK_SYS_GetBusClockFreq (Thumb, 26 bytes, Stack size 8 bytes, fsl_clock_mk60d10.o(i.CLOCK_SYS_GetBusClockFreq))
  [Stack]

  - Max Depth = 92
  - Call Chain = CLOCK_SYS_GetBusClockFreq ⇒ CLOCK_HAL_GetOutClk ⇒ CLOCK_HAL_GetFllClk ⇒ CLOCK_HAL_GetFllRefClk ⇒ CLOCK_HAL_TestFllExternalRefFreq
  [Calls]
  - >> CLOCK_HAL_GetOutClk
  [Called By]
  - >> CLOCK_SYS_GetUartFreq

  CLOCK_SYS_GetCoreClockFreq (Thumb, 24 bytes, Stack size 8 bytes, fsl_clock_mk60d10.o(i.CLOCK_SYS_GetCoreClockFreq))
  [Stack]

  - Max Depth = 92
  - Call Chain = CLOCK_SYS_GetCoreClockFreq ⇒ CLOCK_HAL_GetOutClk ⇒ CLOCK_HAL_GetFllClk ⇒ CLOCK_HAL_GetFllRefClk ⇒ CLOCK_HAL_TestFllExternalRefFreq
  [Calls]
  - >> CLOCK_HAL_GetOutClk
  [Called By]
  - >> CLOCK_SYS_SetConfiguration
  - >> CLOCK_SYS_FllStableDelay

  CLOCK_SYS_GetSystemClockFreq (Thumb, 24 bytes, Stack size 8 bytes, fsl_clock_mk60d10.o(i.CLOCK_SYS_GetSystemClockFreq))
  [Stack]

  - Max Depth = 92
  - Call Chain = CLOCK_SYS_GetSystemClockFreq ⇒ CLOCK_HAL_GetOutClk ⇒ CLOCK_HAL_GetFllClk ⇒ CLOCK_HAL_GetFllRefClk ⇒ CLOCK_HAL_TestFllExternalRefFreq
  [Calls]
  - >> CLOCK_HAL_GetOutClk
  [Called By]
  - >> CLOCK_SYS_GetUartFreq

  CLOCK_SYS_GetUartFreq (Thumb, 46 bytes, Stack size 8 bytes, fsl_clock_mk60d10.o(i.CLOCK_SYS_GetUartFreq))
  [Stack]

  - Max Depth = 100
  - Call Chain = CLOCK_SYS_GetUartFreq ⇒ CLOCK_SYS_GetSystemClockFreq ⇒ CLOCK_HAL_GetOutClk ⇒ CLOCK_HAL_GetFllClk ⇒ CLOCK_HAL_GetFllRefClk ⇒ CLOCK_HAL_TestFllExternalRefFreq
  [Calls]
  - >> CLOCK_SYS_GetSystemClockFreq
  - >> CLOCK_SYS_GetBusClockFreq
  [Called By]
  - >> DbgConsole_Init

  CLOCK_SYS_OscInit (Thumb, 160 bytes, Stack size 16 bytes, fsl_clock_manager.o(i.CLOCK_SYS_OscInit))
  [Stack]

  - Max Depth = 160 + Unknown Stack Size
  - Call Chain = CLOCK_SYS_OscInit ⇒ __aeabi_assert ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> __aeabi_assert
  - >> OSC_HAL_SetCapacitor
  - >> CLOCK_HAL_SetOsc0Mode
  - >> CLOCK_SYS_SetOscerConfigration
  [Called By]
  - >> BOARD_InitOsc0

  CLOCK_SYS_RtcOscInit (Thumb, 204 bytes, Stack size 24 bytes, fsl_clock_manager.o(i.CLOCK_SYS_RtcOscInit))
  [Stack]

  - Max Depth = 168 + Unknown Stack Size
  - Call Chain = CLOCK_SYS_RtcOscInit ⇒ __aeabi_assert ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> __aeabi_assert
  - >> RTC_HAL_SetOscillatorCmd
  [Called By]
  - >> BOARD_InitRtcOsc

  CLOCK_SYS_SetConfiguration (Thumb, 72 bytes, Stack size 16 bytes, fsl_clock_mk60d10.o(i.CLOCK_SYS_SetConfiguration))
  [Stack]

  - Max Depth = 160 + Unknown Stack Size
  - Call Chain = CLOCK_SYS_SetConfiguration ⇒ __aeabi_assert ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> __aeabi_assert
  - >> CLOCK_HAL_SetOutDiv
  - >> CLOCK_SYS_GetCoreClockFreq
  - >> CLOCK_SYS_SetSimConfigration
  - >> CLOCK_SYS_SetOscerConfigration
  - >> CLOCK_SYS_SetMcgMode
  [Called By]
  - >> BOARD_ClockInit

  CLOCK_SYS_SetMcgMode (Thumb, 340 bytes, Stack size 40 bytes, fsl_clock_manager.o(i.CLOCK_SYS_SetMcgMode))
  [Stack]

  - Max Depth = 112
  - Call Chain = CLOCK_SYS_SetMcgMode ⇒ CLOCK_HAL_SetPbeMode ⇒ CLOCK_HAL_GetMcgMode
  [Calls]
  - >> CLOCK_HAL_UpdateFastClkInternalRefDiv
  - >> CLOCK_HAL_SetPbeMode
  - >> CLOCK_HAL_SetFbiMode
  - >> CLOCK_HAL_SetFbeMode
  - >> CLOCK_HAL_GetMcgMode
  - >> CLOCK_HAL_EnablePll0InFllMode
  - >> CLOCK_SYS_SetMcgPeeToFbe
  - >> CLOCK_HAL_SetLowPowerModeCmd
  - >> CLOCK_HAL_SetClkOutSrc
  - >> CLOCK_HAL_GetClkOutStat
  [Called By]
  - >> CLOCK_SYS_SetConfiguration

  CLOCK_SYS_SetOscerConfigration (Thumb, 32 bytes, Stack size 16 bytes, fsl_clock_manager.o(i.CLOCK_SYS_SetOscerConfigration))
  [Stack]

  - Max Depth = 16
  - Call Chain = CLOCK_SYS_SetOscerConfigration
  [Calls]
  - >> OSC_HAL_SetExternalRefClkInStopModeCmd
  - >> OSC_HAL_SetExternalRefClkCmd
  [Called By]
  - >> CLOCK_SYS_SetConfiguration
  - >> CLOCK_SYS_OscInit

  DbgConsole_Init (Thumb, 158 bytes, Stack size 48 bytes, fsl_debug_console.o(i.DbgConsole_Init))
  [Stack]

  - Max Depth = 200 + Unknown Stack Size
  - Call Chain = DbgConsole_Init ⇒ CLOCK_SYS_EnableUartClock ⇒ __aeabi_assert ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> UART_HAL_SetParityMode
  - >> UART_HAL_SetBaudRate
  - >> CLOCK_SYS_GetUartFreq
  - >> CLOCK_SYS_EnableUartClock
  - >> __aeabi_memcpy4
  [Called By]
  - >> dbg_uart_init

  OSC_HAL_SetCapacitor (Thumb, 12 bytes, Stack size 0 bytes, fsl_osc_hal.o(i.OSC_HAL_SetCapacitor))
  [Called By]

  - >> CLOCK_SYS_OscInit

  SystemInit (Thumb, 22 bytes, Stack size 0 bytes, system_mk60d10.o(i.SystemInit))
  [Address Reference Count : 1]

  - startup_mk60d10.o(.text)

  UART_HAL_Getchar (Thumb, 12 bytes, Stack size 0 bytes, fsl_uart_hal.o(i.UART_HAL_Getchar))
  [Called By]

  - >> UART_HAL_ReceiveDataPolling

  UART_HAL_Putchar (Thumb, 10 bytes, Stack size 0 bytes, fsl_uart_hal.o(i.UART_HAL_Putchar))
  [Called By]

  - >> UART_HAL_SendDataPolling

  UART_HAL_ReceiveDataPolling (Thumb, 86 bytes, Stack size 24 bytes, fsl_uart_hal.o(i.UART_HAL_ReceiveDataPolling))
  [Stack]

  - Max Depth = 24
  - Call Chain = UART_HAL_ReceiveDataPolling
  [Calls]
  - >> UART_HAL_Getchar
  [Address Reference Count : 1]
  - fsl_debug_console.o(i.DbgConsole_Init)

  UART_HAL_SendDataPolling (Thumb, 46 bytes, Stack size 16 bytes, fsl_uart_hal.o(i.UART_HAL_SendDataPolling))
  [Stack]

  - Max Depth = 16
  - Call Chain = UART_HAL_SendDataPolling
  [Calls]
  - >> UART_HAL_Putchar
  [Address Reference Count : 1]
  - fsl_debug_console.o(i.DbgConsole_Init)

  UART_HAL_SetBaudRate (Thumb, 68 bytes, Stack size 16 bytes, fsl_uart_hal.o(i.UART_HAL_SetBaudRate))
  [Stack]

  - Max Depth = 16
  - Call Chain = UART_HAL_SetBaudRate
  [Called By]
  - >> DbgConsole_Init

  UART_HAL_SetParityMode (Thumb, 28 bytes, Stack size 0 bytes, fsl_uart_hal.o(i.UART_HAL_SetParityMode))
  [Called By]

  - >> DbgConsole_Init

  __aeabi_assert (Thumb, 22 bytes, Stack size 16 bytes, fsl_misc_utilities.o(i.__aeabi_assert))
  [Stack]

  - Max Depth = 144 + Unknown Stack Size
  - Call Chain = __aeabi_assert ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> __2printf
  [Called By]
  - >> CLOCK_SYS_EnablePortClock
  - >> PORT_HAL_SetMuxMode
  - >> CLOCK_SYS_SetConfiguration
  - >> CLOCK_SYS_RtcOscInit
  - >> CLOCK_SYS_OscInit
  - >> PORT_HAL_SetMuxMode
  - >> CLOCK_SYS_EnableUartClock

  _doprint (Thumb, 1380 bytes, Stack size 152 bytes, print_scan.o(i._doprint))
  [Stack]

  - Max Depth = 192
  - Call Chain = _doprint ⇒ fput_pad
  [Calls]
  - >> mknumstr
  - >> fput_pad
  - >> strlen
  [Called By]
  - >> debug_printf

  configure_uart_pins (Thumb, 64 bytes, Stack size 8 bytes, pin_mux.o(i.configure_uart_pins))
  [Stack]

  - Max Depth = 168 + Unknown Stack Size
  - Call Chain = configure_uart_pins ⇒ PORT_HAL_SetMuxMode ⇒ __aeabi_assert ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> PORT_HAL_SetMuxMode
  [Called By]
  - >> dbg_uart_init

  dbg_uart_init (Thumb, 22 bytes, Stack size 8 bytes, board.o(i.dbg_uart_init))
  [Stack]

  - Max Depth = 208 + Unknown Stack Size
  - Call Chain = dbg_uart_init ⇒ DbgConsole_Init ⇒ CLOCK_SYS_EnableUartClock ⇒ __aeabi_assert ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> configure_uart_pins
  - >> DbgConsole_Init
  [Called By]
  - >> hardware_init

  debug_printf (Thumb, 52 bytes, Stack size 32 bytes, fsl_debug_console.o(i.debug_printf))
  [Stack]

  - Max Depth = 224
  - Call Chain = debug_printf ⇒ _doprint ⇒ fput_pad
  [Calls]
  - >> _doprint
  [Called By]
  - >> main
  - >> fprint

  fprint (Thumb, 20 bytes, Stack size 8 bytes, main.o(i.fprint))
  [Stack]

  - Max Depth = 232
  - Call Chain = fprint ⇒ debug_printf ⇒ _doprint ⇒ fput_pad
  [Calls]
  - >> debug_printf
  [Called By]
  - >> LPTMR0_IRQHandler

  fputc (Thumb, 32 bytes, Stack size 16 bytes, fsl_debug_console.o(i.fputc))
  [Stack]

  - Max Depth = 16
  - Call Chain = fputc
  [Address Reference Count : 1]
  - _printf_char_file.o(.text)

  hardware_init (Thumb, 30 bytes, Stack size 8 bytes, hardware_init.o(i.hardware_init))
  [Stack]

  - Max Depth = 216 + Unknown Stack Size
  - Call Chain = hardware_init ⇒ dbg_uart_init ⇒ DbgConsole_Init ⇒ CLOCK_SYS_EnableUartClock ⇒ __aeabi_assert ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> CLOCK_SYS_EnablePortClock
  - >> dbg_uart_init
  - >> BOARD_ClockInit
  [Called By]
  - >> main

  init_data_bss (Thumb, 54 bytes, Stack size 0 bytes, startup.o(i.init_data_bss))
  [Address Reference Count : 1]

  - startup_mk60d10.o(.text)

  main (Thumb, 20 bytes, Stack size 8 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 232 + Unknown Stack Size
  - Call Chain = main ⇒ debug_printf ⇒ _doprint ⇒ fput_pad
  [Calls]
  - >> hardware_init
  - >> debug_printf
  - >> asmmain
  [Called By]
  - >> __rt_entry_main

  ### Local Symbols

  debug_putc (Thumb, 38 bytes, Stack size 16 bytes, fsl_debug_console.o(i.debug_putc))
  [Stack]

  - Max Depth = 16
  - Call Chain = debug_putc
  [Address Reference Count : 1]
  - fsl_debug_console.o(i.debug_printf)

  fput_pad (Thumb, 48 bytes, Stack size 40 bytes, print_scan.o(i.fput_pad))
  [Stack]

  - Max Depth = 40
  - Call Chain = fput_pad
  [Called By]
  - >> _doprint

  mknumstr (Thumb, 166 bytes, Stack size 36 bytes, print_scan.o(i.mknumstr))
  [Stack]

  - Max Depth = 36
  - Call Chain = mknumstr
  [Called By]
  - >> _doprint

  PORT_HAL_SetMuxMode (Thumb, 48 bytes, Stack size 16 bytes, board.o(i.PORT_HAL_SetMuxMode))
  [Stack]

  - Max Depth = 160 + Unknown Stack Size
  - Call Chain = PORT_HAL_SetMuxMode ⇒ __aeabi_assert ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> __aeabi_assert
  [Called By]
  - >> BOARD_ClockInit

  PORT_HAL_SetMuxMode (Thumb, 48 bytes, Stack size 16 bytes, pin_mux.o(i.PORT_HAL_SetMuxMode))
  [Stack]

  - Max Depth = 160 + Unknown Stack Size
  - Call Chain = PORT_HAL_SetMuxMode ⇒ __aeabi_assert ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> __aeabi_assert
  [Called By]
  - >> configure_uart_pins

  CLOCK_HAL_GetClkOutStat (Thumb, 10 bytes, Stack size 0 bytes, fsl_clock_manager.o(i.CLOCK_HAL_GetClkOutStat))
  [Called By]

  - >> CLOCK_SYS_SetMcgMode
  - >> CLOCK_SYS_SetMcgPeeToFbe

  CLOCK_HAL_SetClkOutSrc (Thumb, 10 bytes, Stack size 0 bytes, fsl_clock_manager.o(i.CLOCK_HAL_SetClkOutSrc))
  [Called By]

  - >> CLOCK_SYS_SetMcgMode
  - >> CLOCK_SYS_SetMcgPeeToFbe

  CLOCK_HAL_SetLowPowerModeCmd (Thumb, 12 bytes, Stack size 0 bytes, fsl_clock_manager.o(i.CLOCK_HAL_SetLowPowerModeCmd))
  [Called By]

  - >> CLOCK_SYS_SetMcgMode

  CLOCK_SYS_SetMcgPeeToFbe (Thumb, 66 bytes, Stack size 8 bytes, fsl_clock_manager.o(i.CLOCK_SYS_SetMcgPeeToFbe))
  [Stack]

  - Max Depth = 8
  - Call Chain = CLOCK_SYS_SetMcgPeeToFbe
  [Calls]
  - >> CLOCK_HAL_SetClkOutSrc
  - >> CLOCK_HAL_GetClkOutStat
  [Called By]
  - >> CLOCK_SYS_SetMcgMode

  OSC_HAL_SetExternalRefClkCmd (Thumb, 10 bytes, Stack size 0 bytes, fsl_clock_manager.o(i.OSC_HAL_SetExternalRefClkCmd))
  [Called By]

  - >> CLOCK_SYS_SetOscerConfigration

  OSC_HAL_SetExternalRefClkInStopModeCmd (Thumb, 10 bytes, Stack size 0 bytes, fsl_clock_manager.o(i.OSC_HAL_SetExternalRefClkInStopModeCmd))
  [Called By]

  - >> CLOCK_SYS_SetOscerConfigration

  RTC_HAL_SetOscillatorCmd (Thumb, 14 bytes, Stack size 0 bytes, fsl_clock_manager.o(i.RTC_HAL_SetOscillatorCmd))
  [Called By]

  - >> CLOCK_SYS_RtcOscInit

  CLOCK_SYS_FllStableDelay (Thumb, 30 bytes, Stack size 8 bytes, fsl_clock_mk60d10.o(i.CLOCK_SYS_FllStableDelay))
  [Stack]

  - Max Depth = 100
  - Call Chain = CLOCK_SYS_FllStableDelay ⇒ CLOCK_SYS_GetCoreClockFreq ⇒ CLOCK_HAL_GetOutClk ⇒ CLOCK_HAL_GetFllClk ⇒ CLOCK_HAL_GetFllRefClk ⇒ CLOCK_HAL_TestFllExternalRefFreq
  [Calls]
  - >> CLOCK_SYS_GetCoreClockFreq
  [Address Reference Count : 1]
  - fsl_clock_mk60d10.o(i.CLOCK_SYS_SetConfiguration)

  CLOCK_SYS_SetSimConfigration (Thumb, 58 bytes, Stack size 16 bytes, fsl_clock_mk60d10.o(i.CLOCK_SYS_SetSimConfigration))
  [Stack]

  - Max Depth = 32
  - Call Chain = CLOCK_SYS_SetSimConfigration ⇒ CLOCK_HAL_SetOutDiv
  [Calls]
  - >> CLOCK_HAL_SetOutDiv
  [Called By]
  - >> CLOCK_SYS_SetConfiguration

  SIM_HAL_EnableClock (Thumb, 34 bytes, Stack size 8 bytes, fsl_clock_mk60d10.o(i.SIM_HAL_EnableClock))
  [Stack]

  - Max Depth = 8
  - Call Chain = SIM_HAL_EnableClock
  [Called By]
  - >> CLOCK_SYS_EnablePortClock
  - >> CLOCK_SYS_EnableUartClock

  CLOCK_HAL_GetInternalRefClkMode (Thumb, 14 bytes, Stack size 0 bytes, fsl_mcg_hal.o(i.CLOCK_HAL_GetInternalRefClkMode))
  [Called By]

  - >> CLOCK_HAL_UpdateFastClkInternalRefDiv

  CLOCK_HAL_GetMcgExternalClkFreq (Thumb, 24 bytes, Stack size 8 bytes, fsl_mcg_hal.o(i.CLOCK_HAL_GetMcgExternalClkFreq))
  [Stack]

  - Max Depth = 8
  - Call Chain = CLOCK_HAL_GetMcgExternalClkFreq
  [Calls]
  - >> CLOCK_HAL_TestOscFreq
  [Called By]
  - >> CLOCK_HAL_GetOutClk
  - >> CLOCK_HAL_GetPll0RefFreq
  - >> CLOCK_HAL_GetFllRefClk

  CLOCK_HAL_SetInternalRefClkMode (Thumb, 12 bytes, Stack size 0 bytes, fsl_mcg_hal.o(i.CLOCK_HAL_SetInternalRefClkMode))
  [Called By]

  - >> CLOCK_HAL_UpdateFastClkInternalRefDiv

  CLOCK_HAL_GetClkOutStat (Thumb, 10 bytes, Stack size 0 bytes, fsl_mcg_hal_modes.o(i.CLOCK_HAL_GetClkOutStat))
  [Called By]

  - >> CLOCK_HAL_SetPbeMode
  - >> CLOCK_HAL_SetFbiMode
  - >> CLOCK_HAL_SetFbeMode
  - >> CLOCK_HAL_GetMcgMode

  CLOCK_HAL_GetFllSrc (Thumb, 14 bytes, Stack size 0 bytes, fsl_mcg_hal_modes.o(i.CLOCK_HAL_GetFllSrc))
  [Called By]

  - >> CLOCK_HAL_SetFbiMode
  - >> CLOCK_HAL_SetFbeMode
  - >> CLOCK_HAL_GetMcgMode

  CLOCK_HAL_GetInternalRefClkMode (Thumb, 14 bytes, Stack size 0 bytes, fsl_mcg_hal_modes.o(i.CLOCK_HAL_GetInternalRefClkMode))
  [Called By]

  - >> CLOCK_HAL_SetFbiMode

  CLOCK_HAL_IsOsc0Stable (Thumb, 22 bytes, Stack size 0 bytes, fsl_mcg_hal_modes.o(i.CLOCK_HAL_IsOsc0Stable))
  [Called By]

  - >> CLOCK_HAL_SetFbeMode
  - >> CLOCK_HAL_PrepareOsc

  CLOCK_HAL_IsPllSelected (Thumb, 22 bytes, Stack size 0 bytes, fsl_mcg_hal_modes.o(i.CLOCK_HAL_IsPllSelected))
  [Called By]

  - >> CLOCK_HAL_SetPbeMode
  - >> CLOCK_HAL_SetFbeMode
  - >> CLOCK_HAL_GetMcgMode

  CLOCK_HAL_PrepareOsc (Thumb, 46 bytes, Stack size 16 bytes, fsl_mcg_hal_modes.o(i.CLOCK_HAL_PrepareOsc))
  [Stack]

  - Max Depth = 16
  - Call Chain = CLOCK_HAL_PrepareOsc
  [Calls]
  - >> CLOCK_HAL_IsOsc0Stable
  [Called By]
  - >> CLOCK_HAL_SetPbeMode

  _printf_input_char (Thumb, 10 bytes, Stack size 0 bytes, _printf_char_common.o(.text))
  [Address Reference Count : 1]

  - _printf_char_common.o(.text)

  ### Undefined Global Symbols